To print one Modular 3D Sine Wave Kit, print:

* 24x "Vertical Axis Unit"
* 9x "Base Segment" (print seventeen if both positive y-axis and negative y-axis should be represented)
* 2x "A1\_Q1"
* 2x "A1\_Q2"
* 2x "A1\_Q3"
* 2x "A1\_Q4"
* 2x "A2\_Q1"
* 2x "A2\_Q2"
* 2x "A2\_Q3"
* 2x "A2\_Q4"
* 2x "A3\_Q1"
* 2x "A3\_Q2"
* 2x "A3\_Q3"
* 2x "A3\_Q4"



NOTE: The above are suggestions for one kit; for advanced variations please use creativity and judgement.



Scale up the models if printing them small is infeasible.

During printing, print the pegs with supports. Here's an example, but trial and error on one grid piece may be prudent. After printing, use needle-nose pliers or a dental pick to remove the supports and be prepared to sand the underside if necessary.
| Setting                    | Value                                                           |
| -------------------------- | --------------------------------------------------------------- |
| **Support type**           | "Everywhere" or "Touching buildplate" (preferred if peg is low) |
| **Support overhang angle** | ≤ 50° (to catch the full underside of the peg and ring)         |
| **Support density**        | 10–20% (enough to hold it up)                                   |
| **Support Z gap**          | 0.1–0.2 mm (ensures supports break away cleanly)                |